{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Directions","Max Ave Conc","Max Abs Conc","Sheet1","zRef_Drop_Downs","MonRoundInfo"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":6,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Directions","index":0,"n_rows":20,"n_cols":2,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"These Guidelines have been transposed from the original \"Resource Recovery Order under Part 9, Clause 93 of the Protection of the Environment Operations (Waste) Regulation 2014\", published by Department of Environment and Climate Change (NSW)."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"The import process is:"]
[null,"1. Import the guidelines appropriate to your project (these are in separate worksheets)"]
[]
[null,"Disclaimer: All care has been exercised in the compilation of these guidelines for quick import to ESDAT, \nhowever no liability is taken for any error.  It is the responsibility of the user to review the contained data \nand ensure their data is compliant with the relevant guidelines, and that this compilation meets their requirements.  "]

{"sheet":"Max Ave Conc","index":1,"n_rows":20,"n_cols":28,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Project:",null,null,"Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","HasLocs"]
["ODBC:",null,null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:"]
[]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Comments","Leached","ActionLevel_Prefix","ActionLevel_Suffix","Conditional_Matrix_Type","Conditional_Depth_From","Conditional_Depth_To","Conditional_ChemCode1","Conditional_ChemCode1_Units","Conditional_ChemCode1_Min_Value_Prefix","Conditional_ChemCode1_Value_Min","Conditional_ChemCode1_Max_Value_Prefix","Conditional_ChemCode1_Value_Max","Conditional_ChemCode2","Conditional_ChemCode2_Units","Conditional_ChemCode2_Min_Value_Prefix","Conditional_ChemCode2_Value_Min","Conditional_ChemCode2_Max_Value_Prefix","Conditional_ChemCode2_Value_Max","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["7439-97-6","Mercury","soil","NSW 2014 Excavated Natural Material (Max Average)",0.5,null,"mg/kg"]
["7440-43-9","Cadmium","soil","NSW 2014 Excavated Natural Material (Max Average)",0.5,null,"mg/kg"]
["7439-92-1","Lead","soil","NSW 2014 Excavated Natural Material (Max Average)",50,null,"mg/kg"]
["7440-38-2","Arsenic","soil","NSW 2014 Excavated Natural Material (Max Average)",20,null,"mg/kg"]
["7440-47-3","Chromium (total)","soil","NSW 2014 Excavated Natural Material (Max Average)",75,null,"mg/kg"]
["7440-50-8","Copper","soil","NSW 2014 Excavated Natural Material (Max Average)",100,null,"mg/kg"]
["7440-02-0","Nickel","soil","NSW 2014 Excavated Natural Material (Max Average)",30,null,"mg/kg"]
["7440-66-6","Zinc","soil","NSW 2014 Excavated Natural Material (Max Average)",150,null,"mg/kg"]
["EC_Lab","Electrical Conductivity (lab)","soil","NSW 2014 Excavated Natural Material (Max Average)",1.5,null,"dS/m"]
["EC_Field","Electrical Conductivity (field)","soil","NSW 2014 Excavated Natural Material (Max Average)",1.5,null,"dS/m"]
["pH_Lab","pH Lab","soil","NSW 2014 Excavated Natural Material (Max Average)",9,5,"-"]
["pH_Field","pH Field","soil","NSW 2014 Excavated Natural Material (Max Average)",9,5,"-"]
["TOTALPAH","Total PAH","soil","NSW 2014 Excavated Natural Material (Max Average)",20,null,"mg/kg"]
["50-32-8","Benzo(a)pyrene","soil","NSW 2014 Excavated Natural Material (Max Average)",0.5,null,"mg/kg"]
["C10-C36","Total Petroleum Hydrocarbons C10 -C36","soil","NSW 2014 Excavated Natural Material (Max Average)",250,null,"mg/kg"]
[null,"Rubber, plastic, bitumen, paper, cloth, paint and wood","soil","NSW 2014 Excavated Natural Material (Max Average)",0.05,null,"%"]

{"sheet":"Max Abs Conc","index":2,"n_rows":24,"n_cols":28,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Project:",null,null,"Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","HasLocs"]
["ODBC:",null,null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:"]
[]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Comments","Leached","ActionLevel_Prefix","ActionLevel_Suffix","Conditional_Matrix_Type","Conditional_Depth_From","Conditional_Depth_To","Conditional_ChemCode1","Conditional_ChemCode1_Units","Conditional_ChemCode1_Min_Value_Prefix","Conditional_ChemCode1_Value_Min","Conditional_ChemCode1_Max_Value_Prefix","Conditional_ChemCode1_Value_Max","Conditional_ChemCode2","Conditional_ChemCode2_Units","Conditional_ChemCode2_Min_Value_Prefix","Conditional_ChemCode2_Value_Min","Conditional_ChemCode2_Max_Value_Prefix","Conditional_ChemCode2_Value_Max","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["7439-97-6","Mercury","soil","NSW 2014 Excavated Natural Material (Absolute Max)",1,null,"mg/kg"]
["7440-43-9","Cadmium","soil","NSW 2014 Excavated Natural Material (Absolute Max)",1,null,"mg/kg"]
["7439-92-1","Lead","soil","NSW 2014 Excavated Natural Material (Absolute Max)",100,null,"mg/kg"]
["7440-38-2","Arsenic","soil","NSW 2014 Excavated Natural Material (Absolute Max)",40,null,"mg/kg"]
["7440-47-3","Chromium (total)","soil","NSW 2014 Excavated Natural Material (Absolute Max)",150,null,"mg/kg"]
["7440-50-8","Copper","soil","NSW 2014 Excavated Natural Material (Absolute Max)",200,null,"mg/kg"]
["7440-02-0","Nickel","soil","NSW 2014 Excavated Natural Material (Absolute Max)",60,null,"mg/kg"]
["7440-66-6","Zinc","soil","NSW 2014 Excavated Natural Material (Absolute Max)",300,null,"mg/kg"]
["EC_Lab","Electrical Conductivity (lab)","soil","NSW 2014 Excavated Natural Material (Absolute Max)",3,null,"dS/m"]
["EC_Field","Electrical Conductivity (field)","soil","NSW 2014 Excavated Natural Material (Absolute Max)",3,null,"dS/m"]
["pH_Lab","pH Lab","soil","NSW 2014 Excavated Natural Material (Absolute Max)",10,4.5,"-"]
["pH_Field","pH Field","soil","NSW 2014 Excavated Natural Material (Absolute Max)",10,4.5,"-"]
["TOTALPAH","Total PAH","soil","NSW 2014 Excavated Natural Material (Absolute Max)",40,null,"mg/kg"]
["50-32-8","Benzo(a)pyrene","soil","NSW 2014 Excavated Natural Material (Absolute Max)",1,null,"mg/kg"]
["71-43-2","Benzene","soil","NSW 2014 Excavated Natural Material (Absolute Max)",0.5,null,"mg/kg"]
["108-88-3","Toluene","soil","NSW 2014 Excavated Natural Material (Absolute Max)",65,null,"mg/kg"]
["100-41-4","Ethyl-benzene","soil","NSW 2014 Excavated Natural Material (Absolute Max)",25,null,"mg/kg"]
["1330-20-7","Xylene","soil","NSW 2014 Excavated Natural Material (Absolute Max)",15,null,"mg/kg"]
["C10-C36","Total Petroleum Hydrocarbons C10 -C36","soil","NSW 2014 Excavated Natural Material (Absolute Max)",500,null,"mg/kg"]
[null,"Rubber, plastic, bitumen, paper, cloth, paint and wood","soil","NSW 2014 Excavated Natural Material (Absolute Max)",0.1,null,"%"]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"zRef_Drop_Downs","index":4,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Table","Column","Values"]

{"sheet":"MonRoundInfo","index":5,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Monitoring_Round"]
["Project_ID"]
["PID"]