{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Directions","STV","LTV","Sheet1","zRef_Drop_Downs","MonRoundInfo"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Directions","index":0,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
[null,"These Guidelines have been transposed from the original."]
[]
[]
[]
[null,"Disclaimer: All care has been exercised in the compilation of these guidelines for quick import to ESDAT, however no liability is taken for any error.  It is the responsibility of the user to review the contained data and ensure their data is compliant with the relevant guidelines, and that this compilation meets their requirements.  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"The import process is:"]
[null,"1. Import using the Import Template required."]
[null,"2. Add any necessary ChemCodes to your database."]

{"sheet":"STV","index":1,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Project:",null,null,"Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","NoLocs"]
["ODBC:",null,null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:"]
[]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Leached","Comments","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["7429-90-5","Aluminium","water","ANZECC 2000 Irrigation Short Term Trigger Values",20,null,"mg/l",0,null,1,1]
["7440-38-2","Arsenic","water","ANZECC 2000 Irrigation Short Term Trigger Values",2,null,"mg/l",0,null,1,1]
["7440-41-7","Beryllium","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.5,null,"mg/l",0,null,1,1]
["7440-43-9","Cadmium","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.05,null,"mg/l",0,null,1,1]
["7440-47-3","Chromium","water","ANZECC 2000 Irrigation Short Term Trigger Values",1,null,"mg/l",0,null,1,1]
["7440-48-4","Cobalt","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-50-8","Copper","water","ANZECC 2000 Irrigation Short Term Trigger Values",5,null,"mg/l",0,null,1,1]
["16984-48-8","Fluoride","water","ANZECC 2000 Irrigation Short Term Trigger Values",2,null,"mg/l",0,null,1,1]
["7439-89-6","Iron","water","ANZECC 2000 Irrigation Short Term Trigger Values",10,null,"mg/l",0,null,1,1]
["7439-92-1","Lead","water","ANZECC 2000 Irrigation Short Term Trigger Values",5,null,"mg/l",0,null,1,1]
["7439-93-2","Lithium","water","ANZECC 2000 Irrigation Short Term Trigger Values",2.5,null,"mg/l",0,"(0.075 Citrus crops)",1,1]
["7439-96-5","Manganese","water","ANZECC 2000 Irrigation Short Term Trigger Values",10,null,"mg/l",0,null,1,1]
["7439-97-6","Mercury","water","ANZECC 2000 Irrigation Short Term Trigger Values",2E-3,null,"mg/l",0,null,1,1]
["7439-98-7","Molybdenum","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.05,null,"mg/l",0,null,1,1]
["7440-02-0","Nickel","water","ANZECC 2000 Irrigation Short Term Trigger Values",2,null,"mg/l",0,null,1,1]
["7782-49-2","Selenium","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.05,null,"mg/l",0,null,1,1]
["7440-61-1","Uranium","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-62-2","Vanadium","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.5,null,"mg/l",0,null,1,1]
["7440-66-6","Zinc","water","ANZECC 2000 Irrigation Short Term Trigger Values",5,null,"mg/l",0,null,1,1]
["7727-37-9","Nitrogen","water","ANZECC 2000 Irrigation Short Term Trigger Values",null,null,"mg/L",0,"25 - 125 Requires site-specific assessment",1,1]
["7723-14-0","Phosphorus","water","ANZECC 2000 Irrigation Short Term Trigger Values",null,null,"mg/L",0,"0.8 - 12 Requires site-specific assessment",1,1]
["pH_Field","pH","water","ANZECC 2000 Irrigation Short Term Trigger Values",8.5,6,"-",0,"for groundwater systems",1,1]
["pH_Lab","pH","water","ANZECC 2000 Irrigation Short Term Trigger Values",8.5,6,"-",0,"for groundwater systems",1,1]
["Radium-226","radium 226","water","ANZECC 2000 Irrigation Short Term Trigger Values",5,null,"Bq/L",0,null,1,1]
["Radium-228","radium 228","water","ANZECC 2000 Irrigation Short Term Trigger Values",2,null,"Bq/L",0,null,1,1]
["Uranium-238","uranium 238","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.2,null,"Bq/L",0,null,1,1]
["Grossalpha","gross alpha","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.5,null,"Bq/L",0,null,1,1]
["Grossbeta","gross beta (excluding k-40)","water","ANZECC 2000 Irrigation Short Term Trigger Values",0.5,null,"Bq/L",0,null,1,1]

{"sheet":"LTV","index":2,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["Project:",null,null,"Table:","[zRef_Environmental_Standards]",null,"Style:","EnviroStandards","NoLocs"]
["ODBC:",null,null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:"]
[]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Leached","Comments","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["7429-90-5","Aluminium","water","ANZECC 2000 Irrigation Long Term Trigger Values",5,null,"mg/l",0,null,1,1]
["7440-38-2","Arsenic","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-41-7","Beryllium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-42-8","Boron","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.5,null,"mg/l",0,null,1,1]
["7440-43-9","Cadmium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.01,null,"mg/l",0,null,1,1]
["7440-47-3","Chromium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-48-4","Cobalt","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.05,null,"mg/l",0,null,1,1]
["7440-50-8","Copper","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.2,null,"mg/l",0,null,1,1]
["16984-48-8","Fluoride","water","ANZECC 2000 Irrigation Long Term Trigger Values",1,null,"mg/l",0,null,1,1]
["7439-89-6","Iron","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.2,null,"mg/l",0,null,1,1]
["7439-92-1","Lead","water","ANZECC 2000 Irrigation Long Term Trigger Values",2,null,"mg/l",0,null,1,1]
["7439-93-2","Lithium","water","ANZECC 2000 Irrigation Long Term Trigger Values",2.5,null,"mg/l",0,"(0.075 Citrus crops)",1,1]
["7439-96-5","Manganese","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.2,null,"mg/l",0,null,1,1]
["7439-97-6","Mercury","water","ANZECC 2000 Irrigation Long Term Trigger Values",2E-3,null,"mg/l",0,null,1,1]
["7439-98-7","Molybdenum","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.01,null,"mg/l",0,null,1,1]
["7440-02-0","Nickel","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.2,null,"mg/l",0,null,1,1]
["7782-49-2","Selenium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.02,null,"mg/l",0,null,1,1]
["7440-61-1","Uranium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.01,null,"mg/l",0,null,1,1]
["7440-62-2","Vanadium","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.1,null,"mg/l",0,null,1,1]
["7440-66-6","Zinc","water","ANZECC 2000 Irrigation Long Term Trigger Values",2,null,"mg/l",0,null,1,1]
["7727-37-9","Nitrogen","water","ANZECC 2000 Irrigation Long Term Trigger Values",5,null,"mg/L",0,null,1,1]
["7723-14-0","Phosphorus","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.05,null,"mg/L",0,"To minimise bioclogging of irrigation equipment",1,1]
["pH_Field","pH","water","ANZECC 2000 Irrigation Long Term Trigger Values",8.5,6,"-",0,"for groundwater systems",1,1]
["pH_Lab","pH","water","ANZECC 2000 Irrigation Long Term Trigger Values",8.5,6,"-",0,"for groundwater systems",1,1]
["Radium-226","radium 226","water","ANZECC 2000 Irrigation Long Term Trigger Values",5,null,"Bq/L",0,null,1,1]
["Radium-228","radium 228","water","ANZECC 2000 Irrigation Long Term Trigger Values",2,null,"Bq/L",0,null,1,1]
["Uranium-238","uranium 238","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.2,null,"Bq/L",0,null,1,1]
["Grossalpha","gross alpha","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.5,null,"Bq/L",0,null,1,1]
["Grossbeta","gross beta (excluding k-40)","water","ANZECC 2000 Irrigation Long Term Trigger Values",0.5,null,"Bq/L",0,null,1,1]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"zRef_Drop_Downs","index":4,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Table","Column","Values"]

{"sheet":"MonRoundInfo","index":5,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Monitoring_Round"]
["Project_ID"]
["PID"]